This directory contains the data records from ADOK for the 18  earthquakes use in 
estimating the site response at ADOK.  Being a three-component accelerometer a 
north-south, east-west, and vertical channel are included (labeled 'A N', 'A E',
and 'A Z' respectively) for each earthquake.  Three subfolders are contained: 'Raw'; 
'Corrected'; and 'resp'.  

'Raw' contains the unprocessed, raw waveforms.
'Corrected' contains the instrument corrected waveforms (poles and zeros were removed, FIR
   filters were removed, and instrument sensitivity was accounted for)
'resp' contains the RDSEED output of the Dataless SEED headers that were used to correct 
   the raw wave forms.
   
The ground motion estimation at ADOK for the M5.6 earthquake used exclusively EarthScope 
Transportable Array (TA) stations.  TA waveform data can be obtained from the Incorporated
Research Institutions for Seismology's Data Management Center: http://www.iris.edu/dms/dmc/ 
   
   